September 1, 2007

Randolph Austin Announces the TP 1000 V Peristalic Pump

Variance in each cycle of less than 1% provides accuracy and repeatability

Available exclusively through Randolph Austin for the US market, the TP 1000 V peristaltic pump is German engineered by Tholen Pumpen, and has had great success in the European marketplace for dosing pumps.   


The TP 1000 V is designed as an exact dose, extremely precise, metering or bottling peristaltic pump.  The TP 1000 V can be operated in a semiautomatic mode or be fully integrated through the RS232 as an automatic filling or metering machine.  The TP 1000 V is available with four different rotors that, in combination with the tubing selected, provide a flow range of 1.56 ml per minute with the 1.6 x 1.6 rotor, to 457 ml per minute with the 6.4 x 1.6 rotor.   The TP 1000 V is an excellent choice for laboratories or filling operations that require repeatable and reliable filling or metering applications.

As a stand-alone unit the TP 1000 V can be programmed through the touch screen provided or it can be integrated into a PLC or computer control. The TP 1000 V also provides for a 4-20 mA or 0-10 VDC signal input provided from a variety of sensors and inputs.

This pump brings accuracy into the manufacturing process and is a promising prospect for the US manufacturer. 

For more information, please contact

Gregg LaMontagne
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