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	NEW!
Series DV
Low Cost Timed Automatic Drain Valve


Dwyer Instruments, Inc., the preferred source for your complete range of practical and affordable instrumentation, is announcing the release of its New Series DV Timed Automatic Drain Valve.

The W.E. Anderson Series DV Timed Automatic Drain Valve is an automatic drain system designed to eliminated the need to manually drain water and harmful sediments from your compressed air system, thereby improving the systems performance.  Can be used on receivers, dryers, tanks, and drop legs for sampling and purging a wide variety of liquids.  The DV Series has a heavy-duty motor for operation under adverse conditions and an adjustable timer to meet specific user requirements.  By design, the DV Series eliminates major drawbacks of other compressed air draining systems.  The valve is brass for corrosion resistance and it is a full port ball valve giving maximum and unobstructed flow with no clogging.  A test button allows for the unit to be cycled at any time.  It is mountable in any position for easy plumbing and trouble free operation.  Series DV Timed Automatic Drain Valves are competitively priced starting at $200.00.

To order a free catalog or for more information, contact Dwyer Instruments, Inc., P.O. Box 373, Michigan City, Ind., 46361.  Telephone: (800) 872-9141 or (219) 879-8000; Fax: (219) 872-9057; Internet address: www.dwyer-inst.com; E-mail: lit@dwyer-inst.com.
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