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	NEW!

Series PBLTX
Submersible Level Transmitter Intrinsically Safe



The Mercoid Division of Dwyer Instruments, Inc. is offering a new and robust submersible level transmitter, the PBLTX. The PBLTX is manufactured for years of trouble free service in the harshest applications and is ideal for wastewater, sludge, and slurries. A large diameter 316 SS diaphragm is incorporated in the PBLTX that is non-clogging and damage resistant to floating solids. Unit is UL approved intrinsically safe for wastewater applications that demand this rating per local codes and regulations.


The PBLTX is designed to measure the height of liquid above its position in the tank, sump, or pit. Featured in the PBLTX is a standoff plate so that the unit can be dropped to the bottom of the tank and 0.25% accuracy. The cable is vented to atmosphere for barometric pressure compensation and can be bought in ETFE or polyurethane. The PBLTX is perfectly suited for level monitoring in lift stations and industrial sumps.

Complete details are available on our website @ http://www.dwyer-inst.com/htdocs/level/SeriesPBLT2Price.cfm#CRA
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